Process for Cleaning Newport Motors

Before any re-lubrication, you need to clean the stage. Use q-tips to clean the rail and the lead screw.  You would want to move the stage so both sides of the rail are cleaned.  After cleaning, apply small droplet of lubricant (Kluber is preferred and used in Newport’s service department) on the rail and on three positions on the lead screw.  Move the stage so the lubricant is distributed along the rail and on the lead screw.

Technical Support at Newport: (for future questions)

**Eftekhari, Ali** <Ali.Eftekhari@newport.com>